121DRK.1-I982
ROVASI IP20 Recessed linear downlights DRAK 100


Power: 17.07 W
Constant Current: 500 mA
Luminous flux: 2520lm
Luminous flux of the fixture: 2444lm
CRI: 80
Colour Temperature: 4000K
Chromaticity Tolerance: MacAdam 3
Beam Angle: 31º
LOR: 97%
Average Service Life: 50000h
LED reliability: >54000h L80B10
UGR: <19
Cd/Klm: 2060
Luminous efficacy: 143 lm/W
lmax: 5191 Cd
This product contains a light source of energy efficiency class C.
Class: 1
IP: 20
Glow wire test: 650º
Embedding dimensions: (602+x)x(78+y)mm
Luminaire dimensions: (602+x)x(78+y)mm
Height: 105mm

Fixture features:
Recessed ceiling mounted linear downlights with symmetrical light distribution to achieve an effective task or general lighting.

Specially developed to solve the installation difficulties in the process of replacing linear luminaires using old fluorescent lamps.

Customized exterior dimensions depending on the installation needs.

Powder painted extruded aluminium profile available in assorted finishes, customized RAL under request.
The adaptation sheet is fixed to the light fixture to create a single body for easier installation.

Range of PMMA optics to achieve specific photometric results.

Highly efficient linear printed circuit board.

Built-in driver, included.

Electronic standard options for lighting control: DALI/DSI.

Passive temperature management.

Ceiling-mounted using galvanized steel support with screws.

Pre-wiring of 35cm cable 3x1mm2.
.

Electronic Options:
S: On/Off 
D: DALI/DSI/switchDIM
There are accessories available for dimming devices.

Finishes:
1: RAL9010: Pure White, 2: RAL9005: Jet Black, 4: RAL7016: Anthracite Grey, 7: RAL9006: White Aluminium
