220KRM.4-I723
ROVASI Inclined IP66 Bollards KORAMU 200


Power: 6 W
Constant Current: 150 mA
Luminous flux: 1165lm
Luminous flux of the fixture: 525lm
CRI: 80
Colour Temperature: 2700K
Chromaticity Tolerance: MacAdam 3
Beam Angle: 91º
LOR: 45%
Average Service Life: 50000h
LED reliability: >60000h L80B10
Luminous efficacy: 87 lm/W
Energy efficiency class: A++
Class: 1
IP: 66
IK: 10
Glow wire test: 850º
Luminaire dimensions: 62x65mm
Weight: 2.4Kg
Height: 660mm
Electronic Equipment:
Bollard with frontal light emission, symmetrical distribution.

Bollard height 602mm with 60º inclination from the horizontal axis.

Protection rating against dust and moisture: IP66 – full protection.

Protection rating for resistance against harmful mechanical impacts: IK10.

Extruded aluminium profile coated with polyester powder along with C4 treatment for corrosion resistance to guarantee further durability. Textured paint finish.
Different RAL colour finishes available under request. 
C5-M special coating for highly corrosive environments is available under request.   


4mm frontal polycarbonate diffuser.

Interior opal diffuser.

Anticondensation device.

Silicone gasket.

Highly efficient linear printed circuit board.

Built-in driver included.

Electronic options for light control: DALI/DSI.
A4 stainless steel locking screw. Optional supply of A2 stainless steel vandal-resistant screws.

IP68 connector not included, it can be ordered separately: F3.A3 (On/Off) / F3.A5 (DALI).
Pre-wiring of 35cm cable 3x1mm2.

Mounting plate for floor installation supplied with the fixture.

.
Electronic Options:
S: On/Off 
D: DALI/DSI/switchDIM
There are accessories available for dimming devices.
Finishes:
1: RAL9010: Pure White, 2: RAL9005: Black Jet, 2: RAL9005: Jet Black, 4: RAL7016: Anthracite Grey, 7: RAL9006: White AluminiumAccessory for concrete installation reference F3.P1.KRM.

Accessory for grass installation reference F3.P1.KRM.

