150KBR.11-I1209
ROVASI  KIBRI 100


Power: 6.7 W
Constant Current: 250 mA
Luminous flux: 885lm
Luminous flux of the fixture: 867lm
CRI: 80
Colour Temperature: 3000K
Chromaticity Tolerance: MacAdam3
Beam Angle: 78º
LOR: 98%
Average Service Life: 50000h
LED reliability: >90.000h L80B10
UGR: <19
Luminous efficacy: 129 lm/W
This product contains a light source of energy efficiency class C.
Class: 1
IP: 20
Glow wire test: 650º
Embedding dimensions: 293x57mm
Luminaire dimensions: 310x70mm
Height: 90mm

Fixture features:
Recessed ceiling mounted linear downlights with symmetrical light distribution to achieve an effective task or general lighting.
Linear fixture in 310mm length and in a width of 70mm.
Powder painted extruded aluminium profile available in assorted finishes, customized RAL under request.
White finish modular optics in 7 cells designed to ensure visual comfort.
Highly efficient linear printed circuit board.
Built-in driver, included.
Electronic options for lighting control: DALI/DSI.
Passive temperature management.
Ceiling-mounted using steel support with screws.It is possible to combine different lengths and junction modules in different ways to create customized design.

Electronic Options:
S: On/Off 
D: DALI/DSI/switchDIM
There are accessories available for dimming devices.

Finishes:
11: White frame - white reflectorBlind covers available with a length of 280mm or its multiples: accessory reference M5.Y.

