153TRT.1-I615
ROVASI  TIRET 100


Power: 38.6 W
Luminous flux: 4500lm
Luminous flux of the fixture: 2610lm
CRI: >90
Colour Temperature: 2700K - 6500K
Beam Angle: 84º
Average Service Life: 50000h
This product contains a light source of energy efficiency class F.
Class: 1
IP: 40
Glow wire test: 650º
Embedding dimensions: 847x43mm
Luminaire dimensions: 862x54mm
Weight: 2.39Kg
Height: 75mm

Fixture features:
Recessed  linear downlights with symmetrical light distribution to achieve an effective task or general lighting.
Linear fixture in 846mm length and in a width of 40mm.
Powder painted extruded aluminium profile available in assorted finishes, customized RAL under request.
Opal extruded polycarbonate diffuser.
Highly efficient linear printed circuit board.
Accessories available to create customized linear systems.
Built-in driver, included. Tunable White: 2700K - 6500K.
Electronic options for lighting control: DALI/DSI.
Passive temperature management.
Ceiling-mounted using galvanized steel support with screws.

It is possible to combine different lengths and junction modules in different ways to create customized systems.

Electronic Options:
T: SwitchDIM/ColourSwitch/DALI/DSI
There are available accessories for dimming devices.

Finishes:
1: RAL9010: Pure White, 2: RAL9005: Jet Black, 4: RAL7016: Anthracite Grey, 7: RAL9006: White Aluminium
