456TRT.1-I617
ROVASI  TIRET 400


Power: 59.7 W
Luminous flux: 7500lm
Luminous flux of the fixture: 4350lm
CRI: >90
Colour Temperature: 2700K - 6500K
Beam Angle: 84º
Average Service Life: 50000h
This product contains a light source of energy efficiency class F.
Class: 1
IP: 40
Glow wire test: 650º
Luminaire dimensions: 1406x40mm
Weight: 4.41Kg
Height: 75mm

Fixture features:
Pendant linear downlights with symmetrical light distribution to achieve an effective task or general lighting.
Linear fixture in 1406mm length and in a width of 40mm.
Powder painted extruded aluminium profile available in assorted finishes, customized RAL under request.
Opal extruded polycarbonate diffuser.
Highly efficient linear printed circuit board.
Accessories available to create customized linear systems.
Built-in driver, included. Tunable White: 2700K - 6500K.
Electronic options for lighting control: DALI/DSI.
Emergency kit as option.
Passive temperature management.
Ceiling-mounted with adjustable steel wire suspensoin (1m) and transparent electrical wire. Different suspensoin length on request.

It is possible to combine different lengths and junction modules in different ways to create customized systems.

Electronic Options:
T: SwitchDIM/ColourSwitch/DALI/DSI
There are available accessories for dimming devices.

Finishes:
1: RAL9010: Pure White, 2: RAL9005: Jet Black, 4: RAL7016: Anthracite Grey, 7: RAL9006: White Aluminium
