551TRT.1-I729
ROVASI  TIRET 500


Power: 7.1 W
Constant Current: 150 mA
Luminous flux: 1080lm
Luminous flux of the fixture: 680lm
CRI: 90
Colour Temperature: 4000K
Chromaticity Tolerance: MacAdam 3
Beam Angle: 91º
LOR: 63%
Average Service Life: 50000h
LED reliability: >72000h L80B10
UGR: <19
Cd/Klm: 443
Luminous efficacy: 96 lm/W
This product contains a light source of energy efficiency class D.
Class: 1
IP: 20
Glow wire test: 650º
Luminaire dimensions: 566x40mm
Weight: 2.75Kg
Height: 75mm

Fixture features:
Pendant linear downlights with symmetrical light distribution to achieve an effective task or general lighting. Double light emission: up and down.
Linear fixture in 566mm length and in a width of 40mm.
Powder painted extruded aluminium profile available in assorted finishes, customized RAL under request.
Opal extruded polycarbonate diffuser.
Highly efficient linear printed circuit board.
Accessories available to create customized linear systems.
Built-in Driver, separate switching up and down.
Electronic options for lighting control: DALI/DSI (for downlight position only).
Passive temperature management.
Ceiling-mounted with adjustable steel wire suspension ( 1m ) and transparent electrical wire. Different suspension length on request.

It is possible to combine different lengths and junction modules in different ways to create customized systems.

Electronic Options:
S: On/Off 
D: DALI/DSI/switchDIM
There are accessories available for dimming devices.

Finishes:
1: RAL9010: Pure White, 2: RAL9005: Jet Black, 4: RAL7016: Anthracite Grey, 7: RAL9006: White Aluminium
