230CLT.4-I1106
ROVASI  COLUTEA 200


Power: 10.6 W
Constant Current: 500 mA
Luminous flux: 1550lm
Luminous flux of the fixture: 186lm
CRI: 80
Colour Temperature: 4000K
Chromaticity Tolerance: MacAdam 4
Beam Angle: 360º
LOR: 12%
Average Service Life: 50000h
LED reliability: 52000h L80B50
Luminous efficacy: 18 lm/W
This product contains a light source of energy efficiency class E.
Class: 1
IP: 66
IK: IK10
Glow wire test: 850º
Luminaire dimensions: 140mm
Weight: 3.85Kg
Height: 300mm

Fixture features:
Bollard with 360º light emission, radial beam.

Bollard head with a diameter of 140mm.

Bollard height : 300mm.

Protection rating against dust and moisture: IP66 – full protection.

Protection rating for resistance against harmful mechanical impacts: IK10.

Die-cast aluminium body and top cover made of die-cast aluminium and extruded aluminium tube coated with polyester powder along with C4 treatment for corrosion resistance to guarantee further durability. Textured paint finish.
Different RAL colour finishes available under request. 
C5-M special coating for highly corrosive environments is available under request.   

5mm extruded polycarbonate diffuser made by resins UV stabilized. Opal finish.

Aluminium disks to get specific photometric results and to increase visual comfort.

A4 stainless steel locking screw. Optional supply of A2 stainless steel vandal-resistant screw.
Silicone gasket.

Anticondensation device.

PCB on the top of the fixture.

Built-in driver included.

Electronic options for light control : DALI.

Pre-wiring with 25cm of 3x1mm2 cable.

Double cable gland entry for installation in series.

IP68 connector not included, it can be ordered separately: F3.A3 (On/Off) / F3.A5 (DALI) 
 Mounting base supplied with the fixture.

Electronic Options:
S: On/Off 
D: DALI
There are accessories available for dimming devices.

Finishes:
1: RAL9010: Pure White textured, 2: RAL9005: Jet Black textured, 4: RAL7016: Anthracite Grey textured, 7: RAL9006: White Aluminium texturedAccessory for installation in concrete reference  F3.P1.BLD 
Accessory for installation in grass  reference  F3.O1.BLD.

