907MOV.1-T1149
ROVASI  MOVE 900 OPTIMAL DISPLAY


Power: 11 W
Constant Current: 350 mA
Luminous flux: 1060lm
Luminous flux of the fixture: 965lm
CRI: >90
Colour Temperature: FRESH MEAT
Chromaticity Tolerance: MacAdam 4
Beam Angle: 12º
LOR: 91%
Average Service Life: 50000h
LED reliability: 50000h L90B50
Energy efficiency class: A
Class: 1
IP: 20
Glow wire test: 850º
Luminaire dimensions: 120mm
Height: 175mm
Electronic Equipment:
Track spots with symmetrical light distribution to achieve an effective task, accent or general lighting.
Special LED module created to be the optimal solution for specific projects.
Cylindrical design in diameter 120mm.
Articulated arm adjustable 0º,15º, 30º, 45º, 60º, 75º and 90º and with 355º rotation around the vertical axis.
Facetted metalized or sandblasted metalized aluminium reflector.
Powder painted aluminium body and arm available in assorted finishes, customized RAL under request. Track adaptor available in white, black or grey.
Optional anti-glare accessories for more visual comfort.
Driver built into the track adaptor. Consult compatible tracks with the track adaptor.
Passive temperature management: heat dissipation flows through aluminium heat sink.
Three-phase tracks  are available as well as accessories to create a custom system.
Electronic Options:
S: On/Off
D: DALI/DSI/switchDIM
B: Bluetooth Casambi
Finishes:
1: RAL9010: Pure White, 2: RAL9005: Jet Black, 4: RAL7016: Anthracite Grey, 7: RAL9006: White Aluminium ( resistant to the glow wire test 750º)
